Enabling Call Forwarding

**To enable call forwarding in phone mode:**

* Press **Menu>Features>Call Forward.**
* Press  **** or  to select the desired forwarding type, and then press the **Enter** soft key.
* Depending on your selection:

	+ If you select **Always** Forward:

		- Press  **** or  , or the **Switch** soft key  to select **Enabled** from the Always Forward field.

		
		- Enter the destination number you want to forward all incoming calls to in theForwardto field.
	+ If you select **Busy** Forward:

		- Press  ****or  , or the **Switch** soft key soft key to select **Enabled** from the Busy Forward field.

		
		- Enter the destination number you want to forward all incoming calls to when the phone is busy in the Forward to field.
	+ If you select **No Answer** Forward:

		- Press  ****or****,or the **Switch** soft key  to select **Enabled** from the No Answer Forward field.

		
		- Enter the destination number you want to forward all unanswered incoming calls to in theForwardto field.
		- Press  ****or****,or the**Switch**soft key to select the ring time to wait before forwarding from the After Ring Time field.

		The default ring time is 12 seconds.
* Press the **Save** soft key to accept the change or the **Back** soft key to cancel.
* The    icon on the status bar indicates that the call forward is enabled.